7.0.0

# scevtstreams

Extract stream information and time windows from picks of an event or solitary picks.

## Description

scevtstreams reads all picks of an event or solitary picks determining the time window between the first pick and the last pick. In addition symmetric asymmetric time margins are added to this time window. It writes the streams that are picked including the determined time window for the event to stdout. This tool gives appropriate input information for scart, fdsnws and capstool [30] for CAPS [3] server (Common Acquisition Protocol Server by gempa GmbH) to dump waveforms from archives based on event data.

Events with origins and picks can be read from database or XML file. Solitary picks can only be read from XML file. The XML files can be generated using scxmldump.

## Output Format

The generated list contains start and end time as well as stream information.

Generic:

    starttime;endtime;stream

Example:

    2019-07-17 02:00:00;2019-07-17 02:10:00;GR.CLL..BHZ

## Examples

1. Get the time windows for an event in the database:

       scevtstreams -E gfz2012abcd -d mysql://sysop:sysop@localhost/seiscomp

2. Get the time windows for one specific event or all events in a XML file. The time windows start 120 s before the first pick and ends 500 s after the last pick:

       scevtstreams -i event.xml -E gfz2012abcd
       scevtstreams -i event.xml

3. Get the time windows from all picks in a XML file which does not contain events or origins:

       scevtstreams -i picks.xml

4. Combine with scart for creating a miniSEED data file from one event. The time window starts and ends 5 minutes before the first and after the last pick, respectively. The data is read from SDS archive and sorted by end time:

       scevtstreams -E gfz2012abcd -d mysql://sysop:sysop@localhost/seiscomp -m 300 |\
       scart -dsvE --list - ~/seiscomp/acquisition/archive > gfz2012abcd-sorted.mseed

5. Download waveforms from FDSN and import into local archive. Include all stations from the contributing networks:

       scevtstreams -E gfz2012abcd -d mysql://sysop:sysop@localhost/seiscomp -m 300 -R --all-stations |\
       scart --list - -I fdsnws://geofon.gfz.de ./my-archive

6. Create lists compatible with fdsnws POST format or capstool [30]:

       scevtstreams -E gfz2012abcd -i event.xml -m 120,500 --fdsnws
       scevtstreams -E gfz2012abcd -i event.xml -m 120,500 --caps

## Module Configuration

`etc/defaults/global.cfg`
`etc/defaults/scevtstreams.cfg`
`etc/global.cfg`
`etc/scevtstreams.cfg`
`~/.seiscomp/global.cfg`
`~/.seiscomp/scevtstreams.cfg`

scevtstreams inherits global options.

## Command-Line Options

scevtstreams [options]

### Generic

-h, --help

  Show help message.

-V, --version

  Show version information.

--config-file arg

  Use alternative configuration file. When this option is used the loading of all stages is disabled. Only the given configuration file is parsed and used. To use another name for the configuration create a symbolic link of the application or copy it. Example: scautopick -> scautopick2.

--plugins arg

  Load given plugins.

-D, --daemon

  Run as daemon. This means the application will fork itself and doesn’t need to be started with &.

--auto-shutdown arg

  Enable/disable self-shutdown because a master module shutdown. This only works when messaging is enabled and the master module sends a shutdown message (enabled with --start-stop-msg for the master module).

--shutdown-master-module arg

  Set the name of the master-module used for auto-shutdown. This is the application name of the module actually started. If symlinks are used, then it is the name of the symlinked application.

--shutdown-master-username arg

  Set the name of the master-username of the messaging used for auto-shutdown. If "shutdown-master-module" is given as well, this parameter is ignored.

### Verbosity

--verbosity arg

  Verbosity level [0..4]. 0:quiet, 1:error, 2:warning, 3:info, 4:debug.

-v, --v

  Increase verbosity level (may be repeated, eg. -vv).

-q, --quiet

  Quiet mode: no logging output.

--component arg

  Limit the logging to a certain component. This option can be given more than once.

-s, --syslog

  Use syslog logging backend. The output usually goes to /var/lib/messages.

-l, --lockfile arg

  Path to lock file.

--console arg

  Send log output to stdout.

--debug

  Execute in debug mode. Equivalent to --verbosity=4 --console=1 .

--log-file arg

  Use alternative log file.

### Database

--db-driver-list

  List all supported database drivers.

-d, --database arg

  The database connection string, format: service://user:pwd@host/database. "service" is the name of the database driver which can be queried with "--db-driver-list".

--config-module arg

  The config module to use.

--inventory-db arg

  Load the inventory from the given database or file, format: [service://]location .

--db-disable

  Do not use the database at all

### Input

-i, --input arg

  Input XML file name. Reads event and picks from the XML file instead of database. Use ‘-’ to read from stdin.

-f, --format arg

  Input format to use (xml [default], zxml (zipped xml), binary). Only relevant with -i.

### Dump

-E, --event arg

  The ID of the event to consider.

--net-sta arg

  Filter read picks by network code or network and station code. Format: NET or NET.STA .

--nslc arg

  Stream list file to be used for filtering read picks by stream code. ‘--net-sta’ will be ignored. One line per stream. Line format: NET.STA.LOC.CHA.

### Output

-m, --margin arg

  Time margin around the picked time window, default is 300. Added before the first and after the last pick, respectively. Use 2 comma-separted values (before,after) for asymmetric margins. Example: 120,300.

-S, --streams arg

  Comma separated list of streams per station to add. Example: BH,SH,HH.

-C, --all-components arg

  Specify whether to use all components (1) or just the picked ones (0). Default: 1.

-L, --all-locations arg

  Specify whether to use all location codes (1) or just the picked ones (0). Default: 1.

--all-stations

  Dump all stations from the same network. If unused, just stations with picks are dumped.

--all-networks

  Dump all networks. If unused, just networks with picks are dumped. This option implies --all-stations, --all-locations, --all-streams, --all-components and will only provide the time window.

-R, --resolve-wildcards flag

  If all components are used, use inventory to resolve stream components instead of using ‘?’ (important when Arclink should be used).

--caps

  Dump in capstool format (Common Acquisition Protocol Server by gempa GmbH).

--fdsnws flag

  Dump in FDSN dataselect webservice POST format.